(export (version D)
  (design
    (source "C:\\Documents and Settings\\Steve\\My Documents\\Multipro-tx\\MultiproV2.3d\\Multipro-txV2-3d.sch")
    (date "05/02/2016 16:35:59")
    (tool "eeschema (2013-07-07 BZR 4022)-stable"))
  (components
    (comp (ref IC1)
      (value ATMEGA328-A)
      (footprint TQFP32)
      (libsource (lib atmel) (part ATMEGA328-A))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BC5C99))
    (comp (ref C2)
      (value 0.1uF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BC5DA8))
    (comp (ref R1)
      (value 10K)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BC5FEA))
    (comp (ref R4)
      (value 1K)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BC6125))
    (comp (ref D1)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BC617C))
    (comp (ref X1)
      (value 16MHz)
      (libsource (lib device) (part CRYSTAL))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BC62D3))
    (comp (ref C4)
      (value 18pF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BC62F4))
    (comp (ref C5)
      (value 18pF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53BC631E))
    (comp (ref U1)
      (value NCP1117ST50T3G)
      (libsource (lib regul) (part NCP1117ST50T3G))
      (sheetpath (names /) (tstamps /))
      (tstamp 53C2ACE9))
    (comp (ref U2)
      (value NCP1117ST33T3G)
      (libsource (lib regul) (part NCP1117ST50T3G))
      (sheetpath (names /) (tstamps /))
      (tstamp 53C2AD08))
    (comp (ref C1)
      (value 22uF)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53C2AE5B))
    (comp (ref C3)
      (value 22uF)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53C2AE76))
    (comp (ref C6)
      (value 22uF)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53C2B150))
    (comp (ref R5)
      (value 2K2)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53C2B787))
    (comp (ref R2)
      (value 2K2)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53C2B990))
    (comp (ref R3)
      (value 1K)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53C2B99F))
    (comp (ref U3)
      (value CYRF6936)
      (libsource (lib device) (part CYRF6936))
      (sheetpath (names /) (tstamps /))
      (tstamp 53C2BF57))
    (comp (ref U4)
      (value A7105)
      (libsource (lib device) (part A7105))
      (sheetpath (names /) (tstamps /))
      (tstamp 53C2C184))
    (comp (ref U5)
      (value NRF24L01)
      (libsource (lib device) (part NRF24L01))
      (sheetpath (names /) (tstamps /))
      (tstamp 53C2C24E))
    (comp (ref U6)
      (value CC2500)
      (libsource (lib device) (part CC2500))
      (sheetpath (names /) (tstamps /))
      (tstamp 53C2C3F4))
    (comp (ref R6)
      (value 1K)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53C2D8C4))
    (comp (ref D2)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 53C2D9F8))
    (comp (ref P1)
      (value ISP)
      (libsource (lib conn) (part CONN_3X2))
      (sheetpath (names /) (tstamps /))
      (tstamp 53C2DBCC))
    (comp (ref P2)
      (value CONN_5)
      (libsource (lib conn) (part CONN_5))
      (sheetpath (names /) (tstamps /))
      (tstamp 53FE5423))
    (comp (ref JP2)
      (value JUMPER)
      (libsource (lib device) (part JUMPER))
      (sheetpath (names /) (tstamps /))
      (tstamp 53FE5887))
    (comp (ref JP4)
      (value JUMPER)
      (libsource (lib device) (part JUMPER))
      (sheetpath (names /) (tstamps /))
      (tstamp 53FE5896))
    (comp (ref SW1)
      (value HEX_DIP)
      (libsource (lib device) (part HEX_DIP))
      (sheetpath (names /) (tstamps /))
      (tstamp 54394777))
    (comp (ref C7)
      (value 0.1uF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 54845FE2))
    (comp (ref R7)
      (value 2K2)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 54DCE006))
    (comp (ref P3)
      (value CONN_2)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 56B4E4CA))
    (comp (ref JP3)
      (value JUMPER)
      (libsource (lib device) (part JUMPER))
      (sheetpath (names /) (tstamps /))
      (tstamp 56B4E4E1))
    (comp (ref R8)
      (value 470)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56B4E6D8))
    (comp (ref SW2)
      (value BIND)
      (libsource (lib device) (part SW_PUSH_4_PIN))
      (sheetpath (names /) (tstamps /))
      (tstamp 56B4EC6E))
    (comp (ref SW3)
      (value RESET)
      (libsource (lib device) (part SW_PUSH_4_PIN))
      (sheetpath (names /) (tstamps /))
      (tstamp 56B4EC7B))
    (comp (ref JP1)
      (value JUMPER)
      (libsource (lib device) (part JUMPER))
      (sheetpath (names /) (tstamps /))
      (tstamp 56B4EFD5)))
  (libparts
    (libpart (lib device) (part A7105)
      (fields
        (field (name Reference) U)
        (field (name Value) A7105)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 3V3) (type input))
        (pin (num 2) (name SCS) (type input))
        (pin (num 3) (name GND) (type input))
        (pin (num 4) (name SCK) (type input))
        (pin (num 5) (name SDIO) (type input))
        (pin (num 6) (name GIO1) (type input))
        (pin (num 7) (name GIO2) (type output))
        (pin (num 8) (name RXEN) (type input))
        (pin (num 9) (name TXEN) (type output))))
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CC2500)
      (fields
        (field (name Reference) U)
        (field (name Value) CC2500)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 3V3) (type input))
        (pin (num 2) (name SI) (type input))
        (pin (num 3) (name SCLK) (type input))
        (pin (num 4) (name SO) (type input))
        (pin (num 5) (name GDO2) (type input))
        (pin (num 6) (name GND) (type input))
        (pin (num 7) (name GDOo) (type input))
        (pin (num 8) (name CSn) (type input))
        (pin (num 9) (name PA_EN) (type input))
        (pin (num 10) (name LNA_EN) (type input))))
    (libpart (lib device) (part CP1)
      (description "Condensateur polarise")
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CRYSTAL)
      (fields
        (field (name Reference) X)
        (field (name Value) CRYSTAL)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib device) (part CYRF6936)
      (fields
        (field (name Reference) U)
        (field (name Value) CYRF6936)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 5.0V) (type input))
        (pin (num 2) (name NCS) (type input))
        (pin (num 4) (name SCK) (type input))
        (pin (num 5) (name GND) (type input))
        (pin (num 6) (name GND) (type input))
        (pin (num 8) (name MOSI) (type input))
        (pin (num 9) (name RST) (type input))
        (pin (num 10) (name MISO) (type input))))
    (libpart (lib device) (part HEX_DIP)
      (fields
        (field (name Reference) SW)
        (field (name Value) HEX_DIP)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type output))
        (pin (num 2) (name C) (type passive))
        (pin (num 3) (name 4) (type output))
        (pin (num 4) (name 2) (type output))
        (pin (num 5) (name C) (type passive))
        (pin (num 6) (name 8) (type output))))
    (libpart (lib device) (part JUMPER)
      (fields
        (field (name Reference) JP)
        (field (name Value) JUMPER)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part NRF24L01)
      (fields
        (field (name Reference) U)
        (field (name Value) NRF24L01)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name GND) (type input))
        (pin (num 2) (name 3V3) (type input))
        (pin (num 3) (name CE) (type input))
        (pin (num 4) (name CSN) (type input))
        (pin (num 5) (name SCK) (type input))
        (pin (num 6) (name MOSI) (type input))
        (pin (num 7) (name MISO) (type input))
        (pin (num 8) (name IRQ) (type NotConnected))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part SW_PUSH_4_Pin)
      (description "Push Button 4 Pin")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH_4_Pin)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type input))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type input))))
    (libpart (lib conn) (part CONN_2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib conn) (part CONN_3X2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_3X2)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))))
    (libpart (lib conn) (part CONN_5)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_5)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))))
    (libpart (lib regul) (part NCP1117ST50T3G)
      (description "NCP1117ST50T3G, 1A Low drop-out regulator, Fixed Output 5V, SOT223")
      (docs http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF)
      (footprints
        (fp SOT223))
      (fields
        (field (name Reference) U)
        (field (name Value) NCP1117ST50T3G)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib atmel) (part ATMEGA168A-A)
      (description "ATMEGA168A, TQFP32, 16k Flash, 1kB SRAM, 512B EEPROM")
      (docs http://www.atmel.com/dyn/resources/prod_documents/doc8271.pdf)
      (fields
        (field (name Reference) IC)
        (field (name Value) ATMEGA168A-A)
        (field (name Footprint) TQFP32)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name "(PCINT19/OC2B/INT1)PD3") (type BiDi))
        (pin (num 2) (name "(PCINT20/XCK/T0)PD4") (type BiDi))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name VCC) (type power_in))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name VCC) (type power_in))
        (pin (num 7) (name "(PCINT6/XTAL1/TOSC1)PB6") (type BiDi))
        (pin (num 8) (name "(PCINT7/XTAL2/TOSC2)PB7") (type BiDi))
        (pin (num 9) (name "(PCINT21/OC0B/T1)PD5") (type BiDi))
        (pin (num 10) (name "(PCINT22/OC0A/AIN0)PD6") (type BiDi))
        (pin (num 11) (name "(PCINT23/AIN1)PD7") (type BiDi))
        (pin (num 12) (name "(PCINT0/CLKO/ICP1)PB0") (type BiDi))
        (pin (num 13) (name "(PCINT1/OC1A)PB1") (type BiDi))
        (pin (num 14) (name "(PCINT2/OC1B/~SS~)PB2") (type BiDi))
        (pin (num 15) (name "(PCINT3/OC2A/MOSI)PB3") (type BiDi))
        (pin (num 16) (name "(PCINT4/MISO)PB4") (type BiDi))
        (pin (num 17) (name "(PCINT5/SCK)PB5") (type BiDi))
        (pin (num 18) (name AVCC) (type power_in))
        (pin (num 19) (name ADC6) (type NotConnected))
        (pin (num 20) (name AREF) (type BiDi))
        (pin (num 21) (name GND) (type power_in))
        (pin (num 22) (name ADC7) (type NotConnected))
        (pin (num 23) (name "(PCINT8/ADC0)PC0") (type BiDi))
        (pin (num 24) (name "(PCINT9/ADC1)PC1") (type BiDi))
        (pin (num 25) (name "(PCINT10/ADC2)PC2") (type BiDi))
        (pin (num 26) (name "(PCINT11/ADC3)PC3") (type BiDi))
        (pin (num 27) (name "(PCINT12/SDA/ADC4)PC4") (type BiDi))
        (pin (num 28) (name "(PCINT14/SCL/ADC5)PC5") (type BiDi))
        (pin (num 29) (name "(PCINT14/~RESET~)PC6") (type BiDi))
        (pin (num 30) (name "(PCINT16/RXD)PD0") (type BiDi))
        (pin (num 31) (name "(PCINT17/TXD)PD1") (type BiDi))
        (pin (num 32) (name "(PCINT18/INT0)PD2") (type BiDi)))))
  (libraries
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\library\\device.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\library\\conn.lib"))
    (library (logical regul)
      (uri "C:\\Program Files\\KiCad\\share\\library\\regul.lib"))
    (library (logical atmel)
      (uri "C:\\Program Files\\KiCad\\share\\library\\atmel.lib")))
  (nets
    (net (code 1) (name GND)
      (node (ref P2) (pin 4))
      (node (ref C7) (pin 2))
      (node (ref SW1) (pin 5))
      (node (ref SW1) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref C4) (pin 1))
      (node (ref X1) (pin 4))
      (node (ref SW3) (pin 4))
      (node (ref SW3) (pin 3))
      (node (ref SW2) (pin 4))
      (node (ref SW2) (pin 3))
      (node (ref D1) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref U6) (pin 6))
      (node (ref U5) (pin 1))
      (node (ref U4) (pin 3))
      (node (ref U3) (pin 6))
      (node (ref U3) (pin 5))
      (node (ref C3) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref C6) (pin 2))
      (node (ref IC1) (pin 21))
      (node (ref IC1) (pin 5))
      (node (ref IC1) (pin 3))
      (node (ref X1) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref D2) (pin 2))
      (node (ref P1) (pin 6)))
    (net (code 2) (name "")
      (node (ref D2) (pin 1))
      (node (ref R6) (pin 2)))
    (net (code 3) (name 3V3)
      (node (ref R5) (pin 2))
      (node (ref U6) (pin 1))
      (node (ref U5) (pin 2))
      (node (ref C7) (pin 1))
      (node (ref U4) (pin 1))
      (node (ref U2) (pin 2))
      (node (ref IC1) (pin 18))
      (node (ref IC1) (pin 6))
      (node (ref P1) (pin 2))
      (node (ref IC1) (pin 4))
      (node (ref R1) (pin 1))
      (node (ref C6) (pin 1)))
    (net (code 4) (name /CC25_CSN)
      (node (ref IC1) (pin 11))
      (node (ref U6) (pin 8)))
    (net (code 5) (name /MISO)
      (node (ref U3) (pin 10))
      (node (ref IC1) (pin 10))
      (node (ref U5) (pin 7))
      (node (ref U6) (pin 4)))
    (net (code 6) (name /SCK)
      (node (ref IC1) (pin 2))
      (node (ref U4) (pin 4))
      (node (ref U6) (pin 3))
      (node (ref U3) (pin 4))
      (node (ref U5) (pin 5)))
    (net (code 7) (name /MOSI)
      (node (ref U5) (pin 6))
      (node (ref IC1) (pin 9))
      (node (ref U6) (pin 2))
      (node (ref U4) (pin 5))
      (node (ref U3) (pin 8)))
    (net (code 8) (name +5V)
      (node (ref U2) (pin 3))
      (node (ref U1) (pin 2))
      (node (ref C3) (pin 1))
      (node (ref U3) (pin 1))
      (node (ref R6) (pin 1)))
    (net (code 9) (name /D11)
      (node (ref P1) (pin 4))
      (node (ref SW1) (pin 4))
      (node (ref IC1) (pin 15)))
    (net (code 10) (name /RESET)
      (node (ref IC1) (pin 29))
      (node (ref SW3) (pin 1))
      (node (ref P1) (pin 5))
      (node (ref R1) (pin 2))
      (node (ref SW3) (pin 2)))
    (net (code 11) (name /D12)
      (node (ref P1) (pin 1))
      (node (ref IC1) (pin 16))
      (node (ref SW1) (pin 3)))
    (net (code 12) (name "")
      (node (ref U4) (pin 7))
      (node (ref U4) (pin 8)))
    (net (code 13) (name "")
      (node (ref U4) (pin 6))
      (node (ref U4) (pin 9)))
    (net (code 14) (name /A7105_CSN)
      (node (ref IC1) (pin 32))
      (node (ref U4) (pin 2)))
    (net (code 15) (name /CC25_LANEN)
      (node (ref U6) (pin 5))
      (node (ref U6) (pin 10)))
    (net (code 16) (name /CC25_PAEN)
      (node (ref U6) (pin 9))
      (node (ref U6) (pin 7)))
    (net (code 17) (name /NRF_CE)
      (node (ref R5) (pin 1))
      (node (ref U5) (pin 3)))
    (net (code 18) (name /NRF_CSN)
      (node (ref U5) (pin 4))
      (node (ref IC1) (pin 12)))
    (net (code 19) (name "")
      (node (ref R8) (pin 1))
      (node (ref P3) (pin 2))
      (node (ref JP3) (pin 2)))
    (net (code 20) (name /PPM_IN)
      (node (ref JP2) (pin 1))
      (node (ref P2) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 21) (name "")
      (node (ref JP3) (pin 1))
      (node (ref P2) (pin 5)))
    (net (code 22) (name "")
      (node (ref JP4) (pin 2))
      (node (ref P3) (pin 1)))
    (net (code 23) (name "")
      (node (ref JP2) (pin 2))
      (node (ref R7) (pin 1)))
    (net (code 24) (name "")
      (node (ref R3) (pin 1))
      (node (ref JP1) (pin 2)))
    (net (code 25) (name /RX)
      (node (ref IC1) (pin 30))
      (node (ref R7) (pin 2)))
    (net (code 26) (name "")
      (node (ref P2) (pin 2))
      (node (ref JP4) (pin 1)))
    (net (code 27) (name /TX)
      (node (ref IC1) (pin 31))
      (node (ref R8) (pin 2)))
    (net (code 28) (name /CYRF_RST)
      (node (ref IC1) (pin 28))
      (node (ref U3) (pin 9)))
    (net (code 29) (name /CYRF_CSN)
      (node (ref U3) (pin 2))
      (node (ref IC1) (pin 13)))
    (net (code 30) (name /A0)
      (node (ref IC1) (pin 23))
      (node (ref SW1) (pin 6)))
    (net (code 31) (name /D10)
      (node (ref SW1) (pin 1))
      (node (ref IC1) (pin 14)))
    (net (code 32) (name /xtl2)
      (node (ref X1) (pin 1))
      (node (ref IC1) (pin 8))
      (node (ref C5) (pin 1)))
    (net (code 33) (name /xtl1)
      (node (ref IC1) (pin 7))
      (node (ref X1) (pin 3))
      (node (ref C4) (pin 2)))
    (net (code 34) (name "")
      (node (ref D1) (pin 1))
      (node (ref SW2) (pin 1))
      (node (ref SW2) (pin 2))
      (node (ref R4) (pin 2)))
    (net (code 35) (name /A3)
      (node (ref IC1) (pin 26)))
    (net (code 36) (name /D3)
      (node (ref IC1) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref JP1) (pin 1)))
    (net (code 37) (name /A4)
      (node (ref IC1) (pin 27)))
    (net (code 38) (name /A2)
      (node (ref IC1) (pin 25)))
    (net (code 39) (name /A1)
      (node (ref IC1) (pin 24)))
    (net (code 40) (name /A6)
      (node (ref IC1) (pin 19)))
    (net (code 41) (name /A7)
      (node (ref IC1) (pin 22)))
    (net (code 42) (name /PB5)
      (node (ref P1) (pin 3))
      (node (ref IC1) (pin 17))
      (node (ref R4) (pin 1)))
    (net (code 43) (name "")
      (node (ref IC1) (pin 20))
      (node (ref C2) (pin 1)))
    (net (code 44) (name "")
      (node (ref U5) (pin 8)))
    (net (code 45) (name /BATT)
      (node (ref C1) (pin 1))
      (node (ref P2) (pin 3))
      (node (ref U1) (pin 3)))))