-- FORMAT  <LineType>|<Msg#>|<Text>  
-- Line Type: Text for Menus (T), List_Text Options (LT), List_Text_Image (LI), Flight Mode (FM), RX Name (RX)
-- NO EMPTY LINES
-- Formmatting at end of line: /c=Center, /r=Right, /b=Bold, /m=menu
LT|0x0001|Off
LT|0x0002|On
-- Ihn/Act List Options
LT|0x0003|Inh
LT|0x0004|Act
--
-- Channel selection for SAFE MODE and GAINS on  FC6250HX
LT|0x000C|Inhibit?
LT|0x000D|Ch5
LT|0x000E|Ch6
LT|0x000F|Ch7
LT|0x0010|Ch8
LT|0x0011|Ch9
LT|0x0012|Ch10
LT|0x0013|Ch11
LT|0x0014|Ch12
--
-- Servo Output values
LT|0x002D|5.5ms
LT|0x002E|11ms
LT|0x002F|22ms
--
-- Gain Multiplier Values
LT|0x0032|1 X
LT|0x0033|2 X
LT|0x0034|4 X
--
LT|0x0035|Inh?
LT|0x0036|Thr
LT|0x0037|Ail
LT|0x0038|Ele
LT|0x0039|Rud
LT|0x003A|Ch5
LT|0x003B|Ch6
LT|0x003C|Ch7
LT|0x003D|Ch8
LT|0x003E|Ch9
LT|0x003F|Ch10
LT|0x0040|Ch11
LT|0x0041|Ch12
LT|0x0042|Ch13
LT|0x0043|Ch14
LT|0x0044|Ch15
LT|0x0045|Ch16
LT|0x0046|Ch17
LT|0x0047|Ch18
LT|0x0048|Ch19
LT|0x0049|Ch20
--
T |0x0040|Roll
T |0x0041|Pitch
T |0x0042|Yaw
T |0x0043|Gain/c/b
T |0x0045|Differential
T |0x0046|Priority
T |0x0049|Output Setup 
T |0x004A|Failsafe
T |0x004B|Main Menu
T |0x004E|Position
--
T |0x0050|Outputs
T |0x0051|Output Channel 1
T |0x0052|Output Channel 2
T |0x0053|Output Channel 3
T |0x0054|Output Channel 4
T |0x0055|Output Channel 5
T |0x0056|Output Channel 6
--
-- FailSafe Options
--LT|0x005E|Inhibit
LT|0x005F|Hold Last
LT|0x0060|Preset
--LT|0x0061|Custom
--
T |0x0071|Proportional
T |0x0072|Integral
T |0x0073|Derivate
--
T |0x0078|FM Channel
--
T |0x0080|Orientation
T |0x0082|Heading
T |0x0085|Frame Rate
T |0x0086|System Setup
T |0x0087|F-Mode Setup
T |0x0088|Enabled F-Modes
T |0x0089|Gain Channel
T |0x008A|Gain Sensitivity/r  -- Right Align
T |0x008B|Panic
T |0x008E|Panic Delay
--
LT|0x008D|560hz
--
-- FC6250HX: Callibration Menu -> Begin..Start, Complete, Done
T |0x0091|Begin 
T |0x0090|Apply
T |0x0092|Start
T |0x0093|Complete
T |0x0094|Done
--
T |0x0097|Factory Reset
T |0x0098|Factory Reset
--
T |0x0099|Advanced Setup
T |0x009A|Capture Failsafe Positions
T |0x009C|Custom Failsafe
--
T |0x009F|Save Settings -- Save & Reboot RX 
--
T |0x00A5|First Time Setup
T |0x00AA|Capture Gyro Gains
T |0x00AD|Gain Channel Select
T |0x00AF|Dynamic
T |0x00B0|Self-Level/Angle Dem
T |0x00B1|Envelope
--
-- Flight Modes List Options 
LT|0x00B5|Inhibit
LT|0x00B6|FM1
LT|0x00B7|FM2
LT|0x00B8|FM3
LT|0x00B9|FM4
LT|0x00BA|FM5
LT|0x00BB|FM6
LT|0x00BC|FM7
LT|0x00BD|FM8
LT|0x00BE|FM9
LT|0x00BF|FM10
--
T |0x00BE|Unknown_BE -- Used in Reset menu (0x0001) while the RX is rebooting
--
T |0x00C7|Calibrate Sensor
T |0x00CA|SAFE/Panic Mode Setup
--
T |0x00CD|Level model and capture attitude/m -- SPECIAL MENU to itself who is not a comment
--
-- RX Orientations for AR631/AR637, Optionally attach an Image + Alt Text to display
LT|0x00CB|Pos 1
LI|0x00CB|rx_pos_1.png|Pilot View: RX Label Up, Pins Back 
LT|0x00CC|Pos 2
LI|0x00CC|rx_pos_2.png|Pilot View: RX Label Left, Pins Back 
LT|0x00CD|Pos 3  
LI|0x00CD|rx_pos_3.png|Pilot View: RX Label Down, Pins Back
LT|0x00CE|Pos 4  
LI|0x00CE|rx_pos_4.png|Pilot View: RX Label Right, Pins Back
LT|0x00CF|Pos 5  
LI|0x00CF|rx_pos_5.png|Pilot View: RX Label UP, Pins to Front
LT|0x00D0|Pos 6  
LI|0x00D0|rx_pos_6.png|Pilot View: RX Label Left, Pins Front 
LT|0x00D1|Pos 7  
LI|0x00D1|rx_pos_7.png|Pilot View: RX Label Down, Pins Front 
LT|0x00D2|Pos 8  
LI|0x00D2|rx_pos_8.png|Pilot View: RX Label Right, Pins Front 
LT|0x00D3|Pos 9  
LI|0x00D3|rx_pos_9.png|Pilot View: RX Label Up, Pins Left
LT|0x00D4|Pos 10 
LI|0x00D4|rx_pos_10.png|Pilot View: RX Label Back, Pins Left 
LT|0x00D5|Pos 11 
LI|0x00D5|rx_pos_11.png|Pilot View: RX Label Down, Pins Left
LT|0x00D6|Pos 12
LI|0x00D6|rx_pos_12.png|Pilot View: RX Label Front, Pins Left 
LT|0x00D7|Pos 13
LI|0x00D7|rx_pos_13.png|Pilot View: RX Label Up, Pins Right 
LT|0x00D8|Pos 14
LI|0x00D8|rx_pos_14.png|Pilot View: RX Label Back, Pins Right 
LT|0x00D9|Pos 15
LI|0x00D9|rx_pos_15.png|Pilot View: RX Label Down, Pins Right 
LT|0x00DA|Pos 16
LI|0x00DA|rx_pos_16.png|Pilot View: RX Label Front, Pins Right 
LT|0x00DB|Pos 17
LI|0x00DB|rx_pos_17.png|Pilot View: RX Label Back, Pins Down 
LT|0x00DC|Pos 18
LI|0x00DC|rx_pos_18.png|Pilot View: RX Label Left, Pins Down 
LT|0x00DD|Pos 19
LI|0x00DD|rx_pos_19.png|Pilot View: RX Label Front, Pins Down 
LT|0x00DE|Pos 20
LI|0x00DE|rx_pos_20.png|Pilot View: RX Label Right, Pins Down 
LT|0x00DF|Pos 21
LI|0x00DF|rx_pos_21.png|Pilot View: RX Label Back, Pins Up 
LT|0x00E0|Pos 22
LI|0x00E0|rx_pos_22.png|Pilot View: RX Label Left, Pins Up 
LT|0x00E1|Pos 23
LI|0x00E1|rx_pos_23.png|Pilot View: RX Label Front, Pins Up 
LT|0x00E2|Pos 24
LI|0x00E2|rx_pos_24.png|Pilot View: RX Label Right, Pins Up 
LT|0x00E3|Pos Invalid
LI|0x00E3|rx_pos_25.png|Cannot detect orientation of RX 
--
T |0x00D1|Receiver will Reboot/b
T |0x00D2|Panic Channel
T |0x00D3|Swashplate
T |0x00D5|Agility
T |0x00D8|Stop
T |0x00DA|SAFE/c/b  -- Center + Bold
T |0x00DB|Stability
T |0x00DC|@ per sec
T |0x00DD|Tail rotor
T |0x00DE|Setup
T |0x00DF|AFR
T |0x00E0|Collective
T |0x00E1|Subtrim
T |0x00E2|Phasing
T |0x00E4|E-Ring
T |0x00E5|Swash Type
T |0x00E6|Travel 
T |0x00E7|Left
T |0x00E8|Right
--
LT|0x00F2|Fixed
LT|0x00F3|Adjustable
--
T |0x00F6|Direction
T |0x00F8|Settings -- ?? validate on a Spektrum radio
T |0x00F9|Gyro settings
T |0x00FE|Stick Priority/c/b
--
T |0x0100|Make sure the model has been
T |0x0101|configured, including wing type,
T |0x0102|reversing, travel, trimmed, etc.
T |0x0103|before continuing setup.
T |0x0104| -- Blank
--
T |0x0106|Any wing type, channel assignment,
T |0x0107|subtrim, or servo reversing changes
T |0x0108|require running through initial
T |0x0109|setup again.
T |0x010A| -- Blank
--
T |0x0190|Relearn Servo Settings
T |0x019C|Enter Receiver Bind Mode
T |0x01AA|Offset
T |0x01D7|SAFE Select Channel
T |0x01DC|AS3X/c/b    -- Center + Bold
T |0x01DD|AS3X Settings
T |0x01DE|AS3X Gains
T |0x01E0|Rate Gains/c/b
T |0x01E2|SAFE Settings
T |0x01E3|SAFE Gains
T |0x01E6|Attitude Trim/c/b
T |0x01E7|Envelope
T |0x01E9|Roll Right
T |0x01EA|Roll Left
T |0x01EB|Pitch Down
T |0x01EC|Pitch Up
T |0x01EE|Thr to Pitch
T |0x01EF|Low Thr to Pitch/c/b
T |0x01F0|High Thr to Pitch/c/b
T |0x01F3|Threshold
T |0x01F4|Angle
T |0x01F6|Failsafe Angles/c/b
T |0x01F8|Safe Mode
T |0x01F9|SAFE Select
T |0x01FC|Panic F-Mode
T |0x01FD|FailSafe Flight Mode  -- Safe Flight Mode
T |0x0201|Throttle
T |0x0204|Hover
T |0x0208|Decay
T |0x0209|Save to Backup
T |0x020A|Restore from Backup
T |0x020D|First Time SAFE Setup
--
-- First time safe setup Page 3 : 
T |0x020E|AS3X gains must be tuned
T |0x020F|and active in SAFE Flight Modes
T |0x0210|to help reduce wobble.
T |0x0211| -- Blank
T |0x0212| -- Blank
T |0x0213| -- Blank
--
-- AS3X orientation Setting menu (Level)
T |0x021A|Set the model level,
T |0x021B|and press Continue.
T |0x021C| -- Blank
T |0x021D| -- Blank
--
-- AS3X orientation Setting menu (Nose down)
T |0x021F|Set the model on its nose,
T |0x0220|and press Continue. If the
T |0x0221|orientation on the next
T |0x0222|screen is wrong go back
T |0x0223|and try again.
--
T |0x0224|Continue
T |0x0226|Angle Limits/c/b
T |0x0227|Other settings
T |0x0229|Set Orientation Manually
--
-- Factory Default Warning 
T |0x022B|WARNING!
T |0x022C|This will reset the
T |0x022D|configuration to factory
T |0x022E|defaults. This does not
T |0x022F|affect the backup config.
T |0x0230| -- Blank
--
-- Backup Warning
T |0x0231|This will overwrite the
T |0x0232|backup memory with your
T |0x0233|current configuartion.
T |0x0234| -- Blank
T |0x0235| -- Blank
--
-- Restore from Backup Warning
T |0x0236|This will overwrite the
T |0x0237|current config with
T |0x0238|that which is in
T |0x0239|the backup memory.
T |0x023A| -- blank line
--
-- Utilities Copy flight modes
T |0x023D|Copy F-Mode Settings
T |0x023E|Source F-Mode
T |0x023F|Target F-Mode
--
T |0x0240|Utilities
--
-- Gain Capture Page
T |0x024C|Gains will be captured on
T |0x024D|Captured gains will be
T |0x024E|Gains on
T |0x024F|were captured and changed
T |0x0250|from Adjustable to Fixed
--
--  Utilities, Copy flight mode  (Copy Confirmation, oveerriding FM)
T |0x0251|Are you sure you want to ovewrite the "Target"
T |0x0252|with the "Source" ? 
T |0x0253| -- Blank
--
T |0x0254|Postive = Up, Negative = Down
--
-- First time safe setup Page 1  (maybe ask to select Flight Mode cannel)
T |0x0255|Before setting up SAFE
T |0x0256|a Flight Mode channel
T |0x0257|most be configured.
--
--  First time safe setup Page 2  (something related for flight mode)
T |0x025A|Select the desired flight mode
T |0x025B|switch position to adjust settings
T |0x025C|for each flight mode
T |0x025D| -- Blank
T |0x025E| -- Blank
--
--  Utilities, Copy flight mode  (Confirm)
T |0x0259|YES 
T |0x0260|WARNING: "Target"
T |0x0261|F-Mode will be overwritten
T |0x0262|by "Source"
--
T |0x0263|Fixed/Adjustable Gains/c/b
T |0x0266|Heading Gain/c/b
T |0x0267|Positive = Nose Up/Roll Right
T |0x0268|Negative = Nose Down/Roll Left
T |0x0269|SAFE - Thr to Pitch
T |0x026A|Use CAUTION for Yaw gain!/b
--
T |0x0300|No compatible DSM RX...
T |0x0301|Waiting for RX to Restart
--
FM|0x8000|Flight Mode/c/b
--
RX|0x0001|AR636
RX|0x0014|SPM4651T
RX|0x0015|AR637T
RX|0x0016|AR637TA
RX|0x0018|FC6250HX
RX|0x0019|AR630
RX|0x001A|AR8360T
RX|0x001B|AR8020T
RX|0x001C|AR10360T
RX|0x001E|AR631

