(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "MULTIRF4IN1SMT" (in_bom yes) (on_board yes)
    (property "Reference" "M" (id 0) (at -12.7 21.59 0)
      (effects (font (size 1.27 1.0795)) (justify left bottom))
    )
    (property "Value" "MULTIRF4IN1SMT" (id 1) (at -12.7 -16.51 0)
      (effects (font (size 1.778 1.5113)) (justify left top))
    )
    (property "Footprint" "Multi:MULTIRF4IN1-SMT" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MULTIRF4IN1SMT_1_0"
      (polyline
        (pts
          (xy -12.7 -15.24)
          (xy 12.7 -15.24)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -12.7 20.32)
          (xy -12.7 -15.24)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 12.7 -15.24)
          (xy 12.7 20.32)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 12.7 20.32)
          (xy -12.7 20.32)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (pin bidirectional line (at 15.24 17.78 180) (length 2.54)
        (name "CE_2401" (effects (font (size 1.27 1.27))))
        (number "CE_2401" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
        (name "CS_2401" (effects (font (size 1.27 1.27))))
        (number "CS_2401" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 15.24 0 180) (length 2.54)
        (name "CS_2500" (effects (font (size 1.27 1.27))))
        (number "CS_2500" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
        (name "CS_6936" (effects (font (size 1.27 1.27))))
        (number "CS_6936" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
        (name "CS_7105" (effects (font (size 1.27 1.27))))
        (number "CS_7105" (effects (font (size 0 0))))
      )
      (pin power_in line (at 15.24 -10.16 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "GND" (effects (font (size 0 0))))
      )
      (pin power_in line (at -15.24 17.78 0) (length 2.54)
        (name "GND@1" (effects (font (size 1.27 1.27))))
        (number "GND@1" (effects (font (size 0 0))))
      )
      (pin power_in line (at -15.24 15.24 0) (length 2.54)
        (name "GND@2" (effects (font (size 1.27 1.27))))
        (number "GND@2" (effects (font (size 0 0))))
      )
      (pin power_in line (at -15.24 5.08 0) (length 2.54)
        (name "GND@3" (effects (font (size 1.27 1.27))))
        (number "GND@3" (effects (font (size 0 0))))
      )
      (pin power_in line (at -15.24 0 0) (length 2.54)
        (name "GND@4" (effects (font (size 1.27 1.27))))
        (number "GND@4" (effects (font (size 0 0))))
      )
      (pin power_in line (at -15.24 -10.16 0) (length 2.54)
        (name "GND@5" (effects (font (size 1.27 1.27))))
        (number "GND@5" (effects (font (size 0 0))))
      )
      (pin power_in line (at -15.24 -12.7 0) (length 2.54)
        (name "GND@6" (effects (font (size 1.27 1.27))))
        (number "GND@6" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 15.24 12.7 180) (length 2.54)
        (name "MISO" (effects (font (size 1.27 1.27))))
        (number "MISO" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
        (name "MOSI" (effects (font (size 1.27 1.27))))
        (number "MOSI" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
        (name "PE1" (effects (font (size 1.27 1.27))))
        (number "PE1" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 15.24 -5.08 180) (length 2.54)
        (name "PE2" (effects (font (size 1.27 1.27))))
        (number "PE2" (effects (font (size 0 0))))
      )
      (pin output line (at -15.24 2.54 0) (length 2.54)
        (name "RF" (effects (font (size 1.27 1.27))))
        (number "RF" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
        (name "RST_CYFR" (effects (font (size 1.27 1.27))))
        (number "RST_CYFR" (effects (font (size 0 0))))
      )
      (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
        (name "SCK" (effects (font (size 1.27 1.27))))
        (number "SCK" (effects (font (size 0 0))))
      )
      (pin power_in line (at 15.24 -12.7 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "VCC" (effects (font (size 0 0))))
      )
    )
  )
)
