Cmp-Mod V01 Created by CvPcb (2013-07-07 BZR 4022)-stable date = 05/02/2016 14:40:56

BeginCmp
TimeStamp = /53C2AE5B;
Reference = C1;
ValeurCmp = 22uF;
IdModule  = c_tant_B;
EndCmp

BeginCmp
TimeStamp = /53BC5DA8;
Reference = C2;
ValeurCmp = 0.1uF;
IdModule  = SM0603_Capa;
EndCmp

BeginCmp
TimeStamp = /53C2AE76;
Reference = C3;
ValeurCmp = 22uF;
IdModule  = c_tant_B;
EndCmp

BeginCmp
TimeStamp = /53BC62F4;
Reference = C4;
ValeurCmp = 18pF;
IdModule  = SM0603_Capa;
EndCmp

BeginCmp
TimeStamp = /53BC631E;
Reference = C5;
ValeurCmp = 18pF;
IdModule  = SM0603_Capa;
EndCmp

BeginCmp
TimeStamp = /53C2B150;
Reference = C6;
ValeurCmp = 22uF;
IdModule  = c_tant_B;
EndCmp

BeginCmp
TimeStamp = /54845FE2;
Reference = C7;
ValeurCmp = 0.1uF;
IdModule  = SM0603_Capa;
EndCmp

BeginCmp
TimeStamp = /53BC617C;
Reference = D1;
ValeurCmp = LED;
IdModule  = LED-0603;
EndCmp

BeginCmp
TimeStamp = /53C2D9F8;
Reference = D2;
ValeurCmp = LED;
IdModule  = LED-0603;
EndCmp

BeginCmp
TimeStamp = /53BC5C99;
Reference = IC1;
ValeurCmp = ATMEGA328-A;
IdModule  = TQFP32;
EndCmp

BeginCmp
TimeStamp = /53FE5887;
Reference = JP1;
ValeurCmp = JUMPER;
IdModule  = c_0603;
EndCmp

BeginCmp
TimeStamp = /53FE5896;
Reference = JP2;
ValeurCmp = JUMPER;
IdModule  = c_0603;
EndCmp

BeginCmp
TimeStamp = /56B4E4E1;
Reference = JP3;
ValeurCmp = JUMPER;
IdModule  = c_0603;
EndCmp

BeginCmp
TimeStamp = /56B4EFD5;
Reference = JP4;
ValeurCmp = JUMPER;
IdModule  = c_0603;
EndCmp

BeginCmp
TimeStamp = /53C2DBCC;
Reference = P1;
ValeurCmp = ISP;
IdModule  = pin_array_3x2;
EndCmp

BeginCmp
TimeStamp = /53FE5423;
Reference = P2;
ValeurCmp = CONN_5;
IdModule  = MOLEX_4455_N2X5;
EndCmp

BeginCmp
TimeStamp = /56B4E4CA;
Reference = P3;
ValeurCmp = CONN_2;
IdModule  = PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /53BC5FEA;
Reference = R1;
ValeurCmp = 10K;
IdModule  = SM0603_Resistor;
EndCmp

BeginCmp
TimeStamp = /53C2B990;
Reference = R2;
ValeurCmp = 2K2;
IdModule  = SM0603_Resistor;
EndCmp

BeginCmp
TimeStamp = /53C2B99F;
Reference = R3;
ValeurCmp = 1K;
IdModule  = SM0603_Resistor;
EndCmp

BeginCmp
TimeStamp = /53BC6125;
Reference = R4;
ValeurCmp = 1K;
IdModule  = SM0603_Resistor;
EndCmp

BeginCmp
TimeStamp = /53C2B787;
Reference = R5;
ValeurCmp = 2K2;
IdModule  = SM0603_Resistor;
EndCmp

BeginCmp
TimeStamp = /53C2D8C4;
Reference = R6;
ValeurCmp = 1K;
IdModule  = SM0603_Resistor;
EndCmp

BeginCmp
TimeStamp = /54DCE006;
Reference = R7;
ValeurCmp = 2K2;
IdModule  = SM0603_Resistor;
EndCmp

BeginCmp
TimeStamp = /56B4E6D8;
Reference = R8;
ValeurCmp = 470;
IdModule  = SM0603_Resistor;
EndCmp

BeginCmp
TimeStamp = /54394777;
Reference = SW1;
ValeurCmp = HEX_DIP;
IdModule  = DIP-6__300;
EndCmp

BeginCmp
TimeStamp = /56B4EC6E;
Reference = SW2;
ValeurCmp = BIND;
IdModule  = SW_PUSH_6x4.5MM;
EndCmp

BeginCmp
TimeStamp = /56B4EC7B;
Reference = SW3;
ValeurCmp = RESET;
IdModule  = Switch_SMT5mm;
EndCmp

BeginCmp
TimeStamp = /53C2ACE9;
Reference = U1;
ValeurCmp = NCP1117ST50T3G;
IdModule  = SOT223;
EndCmp

BeginCmp
TimeStamp = /53C2AD08;
Reference = U2;
ValeurCmp = NCP1117ST33T3G;
IdModule  = SOT223;
EndCmp

BeginCmp
TimeStamp = /53C2BF57;
Reference = U3;
ValeurCmp = CYRF6936;
IdModule  = CYRF6936;
EndCmp

BeginCmp
TimeStamp = /53C2C184;
Reference = U4;
ValeurCmp = A7105;
IdModule  = XL7105-D03B;
EndCmp

BeginCmp
TimeStamp = /53C2C24E;
Reference = U5;
ValeurCmp = NRF24L01;
IdModule  = NRF24L01;
EndCmp

BeginCmp
TimeStamp = /53C2C3F4;
Reference = U6;
ValeurCmp = CC2500;
IdModule  = header_10_2mm;
EndCmp

BeginCmp
TimeStamp = /53BC62D3;
Reference = X1;
ValeurCmp = 16MHz;
IdModule  = crystal_FA238-TSX3225;
EndCmp

EndListe
